Attached is a MSVC 6.0 C++ project.  The project builds a "Code Interface Node" for managing the ASIO sound driver for the Layla 3G hardware available from Echo Audio.

 

1) Build a C/C++ .DLL file via the MSVC 6.0 project file GenMon.DSW

2) Convert this to a "Code Interface Node" with LabView supplied utility

3) Insert the Code Interface Node into the ASIO.vi by right clicking on the CIN icon displayed in the ASIO.vi block diagram.

4) Within LabView, run the ASIO.vi stand alone or include it in higher level .vi's.

 

NOTE:  Your ASIO driver should already be installed prior to step 4 above.

NOTE:  The expected name of the ASIO driver in the registry is "ASIO Echo24", if you have installed with a different name, you will have to modify the hard-code in LAYLA_go:layla.cpp.

 

 

Key files are:

 

ASIO.vi  Labview interface to the Layla 3G via the ASIO sound driver.

GenMonCIN.c  Code interface node top level source code file

GenMon.DSW  Project file for building the code interface node

 

 

